Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring DAD Entries

DAD helps a node to determine if an IPv6 address is not already being used by another node. The address could have been assigned either manually or automatically in a stateful or stateless configuration.

These procedures show how to configure DAD entries:

- Set the DAD Attempts

- Reset the DAD Attempts

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |