Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DCB Administration Guide

Search Scope:

- This Document
- Entire Library

### Default Settings

When DCB is enabled, SEFOS configures each of the DCB features with the following default values.

Priority | Priority Group ID (PGID) | PG Bandwidth Allocation (%) | Priority Flow Control | Application Priority Mapping
--- | --- | --- | --- | ---
0 | 0 | 50 (share with same group) | disable | disable
1 | 0 | 50 (share with same group) | disable | disable
2 | 0 | 50 (share with same group) | disable | disable
3 | 1 | 30 | enable | enable
4 | 2 | 20 (share with same group) | disable | disable
5 | 2 | 20 (share with same group) | disable | disable
6 | 2 | 20 (share with same group) | disable | disable
7 | 15 | Unrestricted (not subject to bandwidth limitation) | disable | disable

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |