Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Purge Interval for an Upstream Interface

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Set the purge interval to 100 seconds.

       SEFOS(config-if)# ip igmp-proxy mrouter-time-out 100
       SEFOS(config-if)# end

3. Review the configuration information.

       SEFOS# show ip igmp-proxy mrouter

       IfName/IfId OperVersion CfgVersion UpTime/VersionExpiryTime PurgeIntvl
       ----------------------------------------------------------------------
       vlan2   /40   IGMPv3     IGMPv3      [0d 00:00:59.96]/0        100

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |