Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable the Report Suppression Interval

1. Configure the report suppression interval.

       SEFOS# configure terminal
       SEFOS(config)# ip igmp snooping report-suppression-interval 8
       SEFOS(config)# end

   Only one report is forwarded within the report forward interval of 8 seconds for a particular group.

2. Review the configuration.

       SEFOS# show ip igmp snooping globals

       Snooping Configuration
       -----------------------------
       IGMP Snooping globally enabled
       IGMP Snooping is operationally enabled
       IGMP Snooping Enhanced mode is disabled
       Transmit Query on Topology Change globally disabled
       Multicast forwarding mode is MAC based
       Proxy globally disabled
       Proxy reporting globally enabled
       Filter is disabled
       Router port purge interval is 125 seconds
       Port purge interval is 260 seconds
       Report forward interval is 8 seconds
       Group specific query interval is 2 seconds
       Reports are forwarded on router ports
       Group specific query retry count is 2
       Multicast VLAN disabled
       Leave config level is Vlan based

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |