Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Configure Network Management From CLI (SER MGT)

1. Log into Oracle ILOM CLI.

   See Log Into Oracle ILOM CLI (SER MGT).

2. Verify that the terminal or terminal emulator has the correct settings.

   See SER MGT Port Configuration Parameters.

3. Connect a terminal or terminal emulator to the serial management port on the switch.

   See Front Panel Components for the location of the serial management port on the switch.

4. Press Enter on the terminal device.

   This action establishes the connection between the terminal device and the switch Oracle ILOM.

   The Oracle ILOM login prompt appears.

       SUNSPnnnnnnnnnn login:

5. Enter the user name and password when prompted.

   The default user is `root` and the default password is `changeme`.

   The Oracle ILOM prompt appears.

       ->

6. Change to the `network` directory.

       -> cd SP/network

   Note - By default, the switch uses DHCP as the IP discovery mode. To use `static` as the IP discovery mode, use the following command.

       -> set ipdiscovery = static

7. Configure an externally accessible IP address on the switch.
   1. Set the pending IP address.

          -> set pendingipaddress=n.n.n.n
          Set ’pendingipaddress’ to ’n.n.n.n’

      For example:

          -> set pendingipaddress=10.7.59.97
          Set ’pendingipaddress’ to ’10.7.59.97’

   2. Set the pending IP gateway.

          -> set pendingipgateway=n.n.n.n
          Set ’pendingipgateway’ to ’n.n.n.n’

      For example:

          -> set pendingipgateway=10.7.59.254
          Set ’pendingipgateway’ to ’10.7.59.254’

   3. Set the pending IP netmask.

          -> set pendingipnetmask=n.n.n.n
          Set ’pendingipnetmask’ to ’n.n.n.n’

      For example:

          -> set pendingipnetmask=255.255.255.0
          Set ’pendingipnetmask’ to ’255.255.255.0’

   4. Commit the changes.

          -> set commitpending=true
          Set ’commitpending’ to ’true’

   5. Set the state to enabled.

          -> set state=enabled
          Set ’state’ to ’enabled’

8. Verify the configuration information that you entered.

       -> show

   The CLI displays information about the switch, including its IP address.

   For example:

       -> show

        /SP/network
           Targets:

           Properties:
               type = Network Configuration
               commitpending = (Cannot show property)
               ipaddress = 10.7.59.97
               ipdiscovery = static
               ipgateway = 10.7.59.254
               ipnetmask = 255.255.255.0
               macaddress = 00:14:4f:6C:5D:E8
               pendingipaddress = 10.7.59.97
               pendingipdiscovery = static
               pendingipgateway = 10.7.59.254
               pendingipnetmask = 255.255.255.0
               state = enabled

           Commands:
               cd
               set
               show

       ->

9. When you are done, exit the switch Oracle ILOM.

       -> exit

10. Consider your next steps.

    - Log into Oracle ILOM web.

      See Log Into Oracle ILOM Web (NET MGT).

    - Log into Oracle ILOM CLI.

      See Log Into Oracle ILOM CLI (NET MGT).

##### Related Information

- Oracle ILOM Overview

- Verify the DHCP-Assigned IP Address and Host Name

- Log Into Oracle ILOM Web (NET MGT)

- Log Into Oracle ILOM CLI (NET MGT)

- Log Into Oracle ILOM CLI (SER MGT)

- Configure Network Management From Web

- Configure Network Management From CLI (NET MGT)

- Log Out of ILOM

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |