Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring LAN Prune Delay

The LAN delay inserted by a router in the `LAN-prune-delay` option expresses the expected message propagation delay on the interface. This delay is used by upstream routers to determine the delayed time interval for a join override message before pruning an interface. If the timer expires without a message, the link is pruned. If you notice that temporary forwarding outages are occurring, you might try increasing this value.

- Enable LAN Prune Delay

- Disable LAN Prune Delay

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |