Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the End IP for the Address Pool

In this example, the address pool is `pool 1`, the network is `12.0.0.0`, the mask is `255.0.0.0`, and the end IP is `12.0.0.0`.

1. Create the address pool.

       SEFOS# configure terminal
       SEFOS(config)# ip dhcp pool 1

2. Configure the network as `12.0.0.0`, mask `255.0.0.0`, and end IP as `12.0.0.100`.

       SEFOS(dhcp-config)# network 12.0.0.0 255.0.0.0 12.0.0.100
       SEFOS(dhcp-config)# end

3. View the end IP value for the address pools.

       SEFOS# show ip dhcp server pools

   The output in switch 1 is:

       Pool Id                      : 1
       -------------------------------------------
       Subnet                        : 12.0.0.0
       Subnet Mask                   : 255.0.0.0
       Lease time                    : 3600 secs
       Utilization threshold         : 75%
       Start Ip                      : 12.0.0.1
       End Ip                        : 12.0.0.100

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |