Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Set the Default Route Propagation

1. On switch 1, enter the configuration mode for the interface.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 1
       SEFOS(config-if)# exit

2. Enter the configuration mode for the router.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.1
       SEFOS(config-router)# exit

3. Set the default route.

       SEFOS(config)# interface vlan 1
       SEFOS(config-if)# ip rip default route originate 10

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |