Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LA Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuration Guidelines

The following guidelines must be met:

- Enable port-channel in the system for LA configuration to take effect.

- If 802.1x is enabled on a port, then enable LA on that port only when the port is in the authorized state. You cannot enable LA on unauthorized ports.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |