Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure VGRP for Topology 1

For this configuration, you must ensure that the following prerequisites are met:

- Interface P2 in switch 1 and switch 2 must be enabled.

- VLAN must be configured.

See Example Topolgy 1 for the topology referenced this procedure.

1. Configure the VLAN in switch 1.

       SEFOS# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/15
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# exit
       SEFOS(config)# vlan 2
       SEFOS(config-VLAN)# ports extreme-ethernet 0/15,0/3
       SEFOS(config-VLAN)# exit
       SEFOS(config)# interface extreme-ethernet 0/3
       SEFOS(config-if)# no shutdown
       SEFOS(config-VLAN)# exit

2. Configure the VLAN in switch 2.

       SEFOS# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/3
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# exit

3. Review the VLAN output in switch 1.

       SEFOS# show vlan id 2
       Vlan database
       -------------------
       Vlan ID             : 2
       Member Ports        : Ex0/3, Ex0/15
       Untagged Ports      : None
       Forbidden Ports     : None
       Name                :
       Status              : Permanent
       --------------------------------------

4. Review the VLAN output in switch 2.

       SEFOS# show vlan id 2
       Vlan database
       -------------------
       Vlan ID             : 2
       Member Ports        : Ex0/3
       Untagged Ports      : None
       Forbidden Ports     : None

       Name                :
       Status              : Dynamic Gvrp
       ---------------------------------------

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |