Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable IPv6 Support

1. Enter Interface Configuration mode for `VLAN 3`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 3

2. Enable IPv6 support in the interface.

   The IPv6 link-local address is automatically configured on the interface when you enable IPv6 processing in the interface. IPv6 support is disabled in an interface by default.

       SEFOS(config-if)# ipv6 enable
       SEFOS(config-if)# exit
       SEFOS(config)# exit

3. Review the IPv6 information of the `VLAN 3` interface.

       SEFOS# show ipv6 interface vlan 3

       vlan3 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::214:4fff:fe6c:560f
           Global unicast address(es):
               fec0::2222:0:1/96
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |