Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DCB Administration Guide

Search Scope:

- This Document
- Entire Library

#### Storage Array Server

In a configuration using DCB with SEFOS switches, an optional storage array (server 2) can be configured. This additional server is only required if the host server will run FCoE. Refer to documentation provided with the storage array server for information about configuring the storage array.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |