Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RMON Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Alarms

The alarm group periodically takes statistical samples from variables in the probe and compares them with the thresholds that have been configured. When a threshold is crossed, an event is generated using the alarm hysteresis mechanism. This section contains procedures that explain how to create or disable alarms.

- Create an Alarm

- Disable an Alarm

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |