Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

#### QSFP Cables

Each QSFP connector on the switch contains four SFP+ 10GbE ports (64 10GbE ports total).

The QSFP ports support the following types of cables:

- 4x10 Gbyte fiber SR

- 4x10 Gbyte to 4 SFP+ 10 Gbyte fiber SR

- 4x10 Gbyte direct attach copper

- 4x10 Gbyte to 4 SFP+ 10 Gbyte direct attach copper

Before installing a QSFP Ethernet cable, identify the type of QSFP Ethernet cable that you are using for the connection.

The passive copper Ethernet cable is a single-part unit, where the cable and the optical tranceiver (cable connector) are a single combined assembly.

The active fiber QSFP Ethernet cable is a dual-part unit, where the cable and the optical tranceiver are separate parts.

##### Related Information

- Install the Switch in the Rack

- Splitter Cables

- SFP+ Cables

- Ethernet Cable Cautions

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |