Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the PMBR Status

A PMBR connects a PIMv6 domain to other multicast-routing domains. Configuring the PMBR status enables or disables the PMBR.

1. Enable PIMv6.

       SEFOS# configure terminal
       SEFOS(config)# set ipv6 pim enable

2. Enable the PMBR status.

       SEFOS(config)# set ip pim pmbr enable

3. In `VLAN 7`, associate the interface with PIMv6 component 1.

       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim componentId 1
       SEFOS(config-if)# end

4. Review the PMBR status.

       SEFOS# show ipv6 pim interface detail

       ...
           PIM Component Id : 1
           PIM domain border : enabled
       ...

5. Review the interface details.

       SEFOS# show ipv6 pim interface detail

       ...
           PIM Component Id : 1
           PIM domain border : disabled
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |