Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

## Create Member Ports

This example shows ports 0/2-5 being added to VLAN 2.

1. Enter the VLAN configuration mode for VLAN 2.

       SEFOS# configure terminal
       SEFOS(config)# vlan 2

2. Add member ports to the VLAN.

       SEFOS(config-vlan)# ports extreme-ethernet 0/2-5 untagged ex 0/3
       SEFOS(config-vlan)# end

   Note - You can use `ex` as a replacement for `extreme-ethernet`, as in the preceding syntax.

   Member ports represent the set of ports permanently assigned to the VLAN egress list. Frames belonging to the specified VLAN are forwarded to the ports in the egress list.

   If one of the port types is not explicitly specified as `untagged`, then all of the ports are configured as `tagged` port types, allowing the transmission of frames with the specified VLAN tag. The `untagged` setting allows the port to transmit the frames without a `vlan` tag. This setting is used for devices that cannot support VLAN.

   In the preceding example, the egress packets for the `extreme-ethernet 0/3` interface are transmitted without the tag, but on all of the other ports, the packets are transmitted with the tag.

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |