Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

### L3 RIP and OSPF Configuration Task Overview

Use these tasks to configure L3 RIP and OSPF implementations of the topology. See L2 and L3 Topology.

Goal | Links
--- | ---
Configure L3 routing using RIP. | Configure Switch `TOR72p-1` for L3 Routing Using RIP Configure Switch `TOR72p-2` for L3 Routing Using RIP Configure Switch `ES1-24p-1` for L3 Routing Using RIP Configure Switch `ES1-24p-2` for L3 Routing Using RIP Verify the L3 RIP Configuration
Configure L3 routing using OSPF. | Configure Switch `TOR72p-1` for L3 Routing Using OSPF Configure Switch `TOR72p-2` for L3 Routing Using OSPF Configure Switch `ES1-24p-1` for L3 Routing Using OSPF Configure Switch `ES1-24p-2` for L3 Routing Using OSPF Verify the L3 OSPF Configuration

##### Related Information

- L2 and L3 Topology

- Configuring L3 Routing Based Topology Using RIP

- Configuring L3 Routing Based Topology Using OSPF

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |