Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DCB Administration Guide

Search Scope:

- This Document
- Entire Library

#### Switch B

Switch B is a third-party DCB capable switch with the following specifications:

- Port 33 is connected to port 2 of switch A.

- VLAN is assigned to port 33.

- Optionally, if switch B supports a Fibre Channel port, that port can be connected to the FC port of a storage array server.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |