Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### QoS Administration Guide

Search Scope:

- This Document
- Entire Library

## Define an ACL and Access Group

1. Define an access list to capture source from a subnet.

       SEFOS# configure terminal
       SEFOS(config)# ip access-list extended 200
       SEFOS(config-ext-nacl)# permit ip 10.123.1.0 255.255.255.0 any
       SEFOS(config-ext-nacl)# exit
       SEFOS(config)# ip access-list extended 210
       SEFOS(config-ext-nacl)# permit ip any any
       SEFOS(config-ext-nacl)# exit

2. Apply the ACL to interface `0/1`.

       SEFOS(config)# interface extreme-ethernet 0/1
       SEFOS(config-if)# ip access-group 200 in
       SEFOS(config-if)# ip access-group 210 in
       SEFOS(config-if)# end

3. Review the access list information for `ip 200`.

       SEFOS# show access-lists ip 200
       Extended IP Access List 200
       -----------------------------
       Filter Priority                 : 1
       Filter Protocol Type            : ANY
       IP address Type                 : IPV4
       Source IP address               : 10.123.1.0
       Source IP address mask          : 255.255.255.0
       Source IP Prefix Length         : 24
       Destination IP address          : 0.0.0.0
       Destination IP address mask     : 0.0.0.0
       Destination IP Prefix Length    : 0
       Flow Identifier                 : 0
       In Port List                    : Ex0/1
       Out Port List                   : NIL
       Filter TOS                      : NIL
       Filter DSCP                     : NIL
       Filter Action                   : Permit
       Status                          : Active

4. Review the access list information for `ip 210`.

       SEFOS# show access-lists ip 210
       Extended IP Access List 210
       -----------------------------
       Filter Priority                : 1
       Filter Protocol Type           : ANY
       IP address Type                : IPV4
       Source IP address              : 0.0.0.0
       Source IP address mask         : 0.0.0.0
       Source IP Prefix Length        : 0
       Destination IP address         : 0.0.0.0
       Destination IP address mask    : 0.0.0.0
       Destination IP Prefix Length   : 0
       Flow Identifier                : 0
       In Port List                   : Ex0/1
       Out Port List                  : NIL
       Filter TOS                     : NIL
       Filter DSCP                    : NIL
       Filter Action                  : Permit
       Status                         : Active

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |