Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the PIMv6 Component

This section contains instructions on how to configure the PIMv6 component. Component 1 is the default component, so it cannot be created or deleted.

- Create a PIMv6 Component

- Set the Mode for the PIMv6 Component

- Configure the RP-Candidate Hold Time

- Configure the RP-Candidate Address

- Configure the RP Static Address

- Create an RP-Set Table

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |