Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuration Guidelines

See Topology Example for information on setting up the topology. You must configure all the switches (SEFOS1 to SEFOS9) using these values before configuring OSPF.

Feature | Default Setting
--- | ---
Stability interval | 40
`translation-role` | candidate
`compatible rfc1583` | Enabled
`abr-type` | standard
`neighbor priority` | 1
`area default-cost` | 10
`area tos` | 0
`area metric` | 10
`area - metric-type` | 1
`area - tos` | 0
`default-information originate always metric` | 10
`default-information originate always metric metric-type` | 2
Authentication | no authentication
`hello-interval` | 10
`retransmit-interval` | 5
`transmit-delay` | 1
`dead-interval` | 40
`tag` | 2
`summary-address` | advertise
`translation` | disabled
`redist-config metric-value` | 10
`redist-config metric-type` | asExttype2
`redist-config tag` | manual
`nssa asbr-default-route translator` | disable

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |