Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Check an Endpoint Using Default Values

- Send IPv6 echo messages with the default values for a ping-related configuration.

  For example:

      SEFOS# ping ipv6 fec0::2222:0:1

      ping6 fec0::2222:0:1 100 bytes of data
      100 bytes from fec0::2222:0:1 : ICMP6_seq = 0
      100 bytes from fec0::2222:0:1 : ICMP6_seq = 1
      100 bytes from fec0::2222:0:1 : ICMP6_seq = 2
      100 bytes from fec0::2222:0:1 : ICMP6_seq = 3
      100 bytes from fec0::2222:0:1 : ICMP6_seq = 4
       --- Ping Statistics ---
      5 Packets Transmitted, 5 Packets Received, 0% Packet Loss

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |