Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## OSPFv3 Configurations

Configure the SEFOS implementation of OSPFv3 through the CLI interface. You can use SNMP to view the changes you make to the configuration.

These sections describe the preliminary configurations of Oracle OSPFv3 and describe only IPv6-related configurations. For information about other configurations that you can use to create interfaces and information about entering CLI configuration modes, see CLI Command Modes. For information on IPv6-related configurations, refer to the Sun Ethernet Fabric Operating System IPv6 Administration Guide. Refer to other feature-related administration guides for detailed information about using specific features used in the example configurations in this guide.

- Default Configuration Values

- SNMP MIB Files

- Creating the Base Configuration

- Enabling IPv6 Support and Assigning IPv6 Addresses

- Configuring IPv6 Static Routes

- Creating the Base Configuration for Example Topologies

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |