Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable Redistribution

1. On switch 1, enter the configuration mode for the router.

       SEFOS# configure terminal
       SEFOS(config)# router rip

2. Disable the output delay.

       SEFOS(config-router)# no redistribute static
       SEFOS(config-router)# end

3. On switch 2, review the RIP route entries for the static routes that were added in switch 1.

   The routes were made unreachable with a metric as infinity (16). The static routes are redistributed into the RIP domain.

       SEFOS# show ip rip database

       10.0.0.0/8  [1]        auto-summary
       10.0.0.0/16 [1]        directly connected, vlan1
       50.0.0.0/8  [16]        via 10.0.0.1, vlan1
       60.0.0.0/8  [16]        via 10.0.0.1, vlan1
       70.0.0.0/8  [16]        via 10.0.0.1, vlan1
       80.0.0.0/8  [16]        via 10.0.0.1, vlan1

4. On switch 2, review the RIP route entries for the redistributed static routes that were deleted from the IP routing table.

       SEFOS# show ip route

       C 10.0.0.0/16 is directly connected, vlan1
       C 30.2.2.0/24 is directly connected, vlan3

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |