Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Configuring PIM

These sections describe how to configure SEFOS PIM and provide examples for using various PIM commands. For additional information about these commands and options, refer to the Sun Ethernet Fabric Operating System CLI Enterprise Reference Manual.

- Sample Topology

- Default Settings

- SEFOS1 Configuration

- SEFOS2 Configuration

- Enable PIM

- Reducing Data Transmission Time Using the SPT

- Monitor the Data Transfer Rate After a Register Stop Message

- Configuring PMBR Status

- Enabling Static RP Configurations

- Associate an Interface to a PIM Component

- Delete a PIM Interface

- Configuring Designated Routers

- Configuring the PIM Override Interval

- Configuring PIM LAN Delay

- Configuring LAN Prune Delay

- Configuring BSR Candidates

- Configuring PIM Query Intervals

- Configuring PIM Join and Prune Messaging

- Managing PIM Components

- Configuring PIM Component Data Routing Modes

- Configuring RP-Candidate Behavior

- Configuring RP Candidate Hold Time

- Configuring Static RPs

- Display RP Details

- Enable PIM Neighbor Recognition

- Display PIM Multicast Information

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |