Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Designated Routers

A DR sets up multicast router entries and sends corresponding JP and Register messages on behalf of directly connected receivers and sources, respectively. When you configure the DR priority value for the PIM interface, the router that is configured with the highest priority value will be the DR.

- Prioritize Router Messaging With PIM DR-Priority

- Restore the Default Router Priority Designation

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |