Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Specified Interfaces To Be Passive

If you don't want to configure all interfaces to be passive, you can specify which interfaces should be passive.

This example configures `VLAN 10` as a passive interface.

1. Identify the interface that should be passive and suppress routing updates.

       SEFOS(config)# interface vlan 10
       SEFOS(config-if)# ipv6 ospf passive-interface
       SEFOS(config-if)# end

2. View the configuration details by executing the following show command.

       SEFOS# show ipv6 ospf interface vlan 10

               Ospfv3  Interface  Information

       Interface Name: vlan10      Interface Id: 41    Area Id: 0.0.0.6
       Local Address: fe80::214:4fff:fe6c:628f         Router Id: 10.0.0.1
       Network Type: BROADCAST     Cost: 1             State: DR
       Designated Router Id: 10.0.0.1      local address: fe80::214:4fff:fe6c:628f
       Backup Designated Router Id: 0.0.0.0       local address: (null)
       Transmit Delay: 1 sec        Priority: 1         IfOptions: 0x0
       Timer intervals configured:
       Hello: 10, Dead: 40, Retransmit: 5, Poll: 120
       Demand Circuit: Disable            Neighbor Probing: Disable
       Nbr Probe Retrans Limit: 10        Nbr Probe Interval: 120
       No Hellos (Passive interface)
       Neighbor Count is: 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |