Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the IGMP Version on an Upstream Interface

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Set the IGMP version to 2.

       SEFOS(config-if)# ip igmp-proxy mrouter-version 2
       SEFOS(config-if)# end

3. Review the configuration information.

       SEFOS# show ip igmp-proxy mrouter

       IfName/IfId OperVersion  CfgVersion UpTime/VersionExpiryTime  PurgeIntvl
       -------------------------------------------------------------------------
       vlan2 /40    IGMPv2       IGMPv2         [0d 00:00:59.96]/0         100

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |