Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

#### Example Topolgy 1

In the first example configuration, three hosts are attached to a single switch. Each device has a node name, an associated port, a MAC address, and an IP address.

The following table contains the details of the topology.

Node | Port | IP Address
--- | --- | ---
Host A | N/A | `12.0.0.10`
Host B | N/A | `12.0.0.20`
Host C | N/A | `12.0.0.30`
Switch 1 | P15 | `12.0.0.1`
P16 |
P3 |

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |