Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the IGMP Query Maximum Response Time

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Set the maximum response time to 200 seconds.

       SEFOS(config-if)# ip igmp query-max-response-time 200
       SEFOS(config-if)# end

3. Review the configuration information.

       SEFOS# show ip igmp interface

        vlan2, line protocol is up
        Internet Address is 12.0.0.1/8
        IGMP is enabled on interface
        Current IGMP router version is 2
        IGMP query interval is 125 seconds
        Last member query response interval is 10 seconds
        IGMP max query response time is 200 seconds
        Robustness value is 3
        IGMP querying router is 12.0.0.1 (this system)
        Fast leave is disabled on this interface
        No multicast groups joined

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |