Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

## Configuring an L2 PVRST Based Topology With Active/Standby Bond on the Servers

These tasks describe how to configure each switch for L2 PVRST Active/Standby on the servers.

- Prepare Switch `ToR72p-1` for L2 PVRST Active/Standby on the Servers

- Prepare Switch `ToR72p-2` for L2 PVRST Active/Standby on the Servers

- Configure Switch `ES1-24p-1` for L2 PVRST Active/Standby on the Servers

- Configure Switch `ES1-24p-2` for L2 PVRST Active/Standby on the Servers

- Verify the L2 PVRST Active/Standby Configuration on the Servers

##### Related Information

- Switches Overview

- Understanding L2 and L3 Implementations

- L2 Based Configuration Example Using PVRST Protocol

- Configuring a Basic L2 PVRST Based Topology

- Configuring an L2 PVRST and LLA Based Topology With Active/Active Bond on the Servers

- L3 RIP and OSPF Configuration Overview

- Configuring L3 Routing Based Topology Using RIP

- Configuring L3 Routing Based Topology Using OSPF

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |