Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable Debug

1. On switch 1, enter the configuration mode for the router.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.1
       SEFOS(config-router)# end

2. Enable the debug level.

       SEFOS# debug ip rip all

       RIP: Sending regular Update over this interface 0
       RIP: Authentication not needed for this interface, So 25 routes can be composed
       RIP: If Agg Rt added to update with metric : 3
       RIP: Sending RIP update through Port 0
       RIP: Sending regular Update over this interface 0
       RIP: Authentication not needed for this interface, So 25 routes can be composed
       RIP: If Agg Rt added to update with metric : 3
       RIP: Sending RIP update through Port 0
       RIP: Sending regular Update over this interface 0
       RIP: Authentication not needed for this interface, So 25 routes can be composed
       RIP: If Agg Rt added to update with metric : 3

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |