Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Network Type

You can specify the OSPF network type to be broadcast, non-broadcast, point-to-multipoint, or point-to-point. The default value is broadcast. The OSPF network type can be configured to a type other than the default for a given media.

This example configures the network type for `VLAN 10` as point-to-point, meaning that it is a network that joins a single pair of routers.

1. Configure the network type through the CLI.

       SEFOS(config)# interface vlan 10
       SEFOS(config-if)# ipv6 ospf network point-to-point
       SEFOS(config-if)# end

2. View the configuration.

       SEFOS# show ipv6 ospf interface vlan 10

               Ospfv3  Interface  Information

       Interface Name: vlan10      Interface Id: 41    Area Id: 0.0.0.6
       Local Address: fe80::214:4fff:fe6c:628f         Router Id: 10.0.0.1
       Network Type: PTOP          Cost: 1             State: PTOP
       Designated Router Id: 0.0.0.0       local address: (null)
       Backup Designated Router Id: 0.0.0.0       local address: (null)
       Transmit Delay: 1 sec        Priority: 1         IfOptions: 0x0
       Timer intervals configured:
       Hello: 10, Dead: 40, Retransmit: 5, Poll: 120
       Demand Circuit: Disable            Neighbor Probing: Disable
       Nbr Probe Retrans Limit: 10        Nbr Probe Interval: 120
       Hello due in 4 sec
       Neighbor Count is: 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |