Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

#### SER MGT Port Configuration Parameters

The terminal device can be an actual terminal, a laptop running a terminal emulator, or a terminal server. The terminal device must be set to the following:

- 8N1: eight data bits, no parity, one stop bit

- 9600 baud (default, can be set to any standard rate up to 57600)

- Disable software flow control (XON/XOFF)

  The cable requires the following pin assignments.

  Pin | Signal Description
  --- | ---
  1 | Request To Send (RTS)
  2 | Data Terminal Ready (DTR)
  3 | Transmit Data (TXD)
  4 | Ground
  5 | Ground
  6 | Receive Data (RXD)
  7 | Data Set Ready (DSR)
  8 | Clear To Send (CTS)

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |