Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Multicast Forwarding Mode

The snooping multicast forwarding mode can be IP-based or MAC-based. By default, multicast forwarding mode is MAC based. In this example, the snooping multicast forwarding mode is IP.

1. Configure the multicast forwarding mode.

       SEFOS# configure terminal
       SEFOS(config)# snooping multicast-forwarding-mode ip
       SEFOS(config)# end

2. View the configuration.

       SEFOS# show ipv6 mld snooping globals

       Snooping Configuration
       -----------------------------
       MLD Snooping globally disabled
       MLD Snooping is operationally disabled
       Multicast forwarding mode is IP based
       Proxy reporting globally enabled
       Router port purge interval is 125 seconds
       Port purge interval is 260 seconds
       Report forward interval is 5 seconds
       Group specific query interval is 2 seconds
       Reports are forwarded on router ports
       Group specific query retry count is 2

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |