Skip Navigation Links
| Sun Ethernet Fabric Operating System ### PVRST+ Administration Guide

Search Scope:

- This Document
- Entire Library

## Sun Ethernet Fabric Operating System

### PVRST+ Administration Guide

#### July 2012

This document describes how to administer PVRST+ software on switches running SEFOS.

- Document Information
- Using This Documentation
  - Product Notes
  - Related Documentation
  - Acronyms and Abbreviations
  - CLI Command Modes
  - Feedback
  - Support and Accessibility
- PVRST+ Overview
  - Protocol Description
  - Topology Example
  - Default Settings
  - Rapid STP
    - Bridge ID and Switch Priority
    - Election of the Root Switch
    - Port States
    - Port Roles
    - Rapid Convergence
    - Proposal Agreement Sequence
    - Topology Change and Topology Change Detection
  - VLAN Module
- Configuring RSTP in PVRST+
  - Enable IPv6 Support and Assign IPv6 Addresses
  - Configure the Spanning-Tree Path Cost
  - Configure the Spanning Tree Link Type
  - Configure the Spanning-Tree `portfast` Setting
  - Configure Spanning Tree Timers
  - Display the Spanning Tree Status
  - Configure the Transmit Hold Count
  - Configure Encapsulation
  - Configure the BPDU Guard
  - Configure the Root Guard
- Configuring the VLAN Module
  - Disable GVRP
  - Configuring Trunk and Access Ports
    - Configure a Trunk Port
    - Configure an Access Port
    - Set Up PVID on a Port
  - Configure VLANS and Display the PVRST+ Information for VLANs

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices