Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

### Electrical Specifications

Parameter | AC Version Requirement
--- | ---
Voltage | 100 VAC to 240 VAC single phase, 47-63 Hz
Current (available per input) | 8.8 A maximum per input

##### Related Information

- Physical Specifications

- Environmental Specifications

- Acoustic Noise Emissions

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |