Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Neighbor Probe Values

You can set the number of consecutive LSA retransmissions before the neighbor is deemed inactive, and can also specify how often the neighbor is probed.

- Configure the Neighbor Probe Retransmission Limit

- Restore the Default Neighbor Probe Retransmission Limit

- Configure the Neighbor Probe Interval

- Restore the Default Neighbor Probe Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |