Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PVRST+ Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure an Access Port

1. Disable GVRP on the port.

   Per-port GVRP must be disabled before configuring as access mode.

       TOR-1 SEFOS# configure terminal
       TOR-1 SEFOS(config)# set port gvrp extreme-ethernet 0/1 disable
       TOR-1 SEFOS(config)#

2. Enter the configuration mode for the interface.

       TOR-1 SEFOS(config)# interface  extreme-ethernet 0/1
       TOR-1 SEFOS(config-if)#

3. Set the `switchport` mode.

       SEFOS(config-if)# switchport acceptable-frame-type   untaggedAndPrioritytagged
       SEFOS(config-if)# switchport mode access
       SEFOS(config-if)# end
       TOR-1 SEFOS#

   After you configure the port as access, the port becomes a member port of the VLAN that is configured as PVID for that port.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |