Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Test Redistribution

1. On switch 1, enter the configuration mode for the router.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.1

2. Enable redistribution.

       SEFOS(config-router)# redistribute static
       SEFOS(config-router)# exit

3. Add static routes.

       SEFOS(config)# ip route 50.0.0.0 255.0.0.0 vlan 2
       SEFOS(config)# ip route 60.0.0.0 255.0.0.0 vlan 2
       SEFOS(config)# ip route 70.0.0.0 255.0.0.0 vlan 2
       SEFOS(config)# ip route 80.0.0.0 255.0.0.0 vlan 2
       SEFOS(config)# end

4. On switch 2, test the redistribution.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.2
       SEFOS(config-router)# end

5. Review the redistribution of static routes on switch 1.

       SEFOS# show ip protocols

       Routing Protocol is rip

       Vrf  default
        RIP2 security level is Maximum
        Redistributing : rip, static
        Output Delay is disabled
        Retransmission timeout interval is 5 seconds
        Number of retransmission retries is 36
        Default metric is 3
        Auto-Summarisation of routes is enabled
        Routing for Networks :
          10.0.0.0
        Routing Information Sources :
        Interface Specific Address Summarization :
        Trusted Neighors :
        Interface vlan1
         Sending updates every 30 seconds
         Invalid after 180 seconds
         Flushed after 120 seconds
         Send version is 1 2, receive version is 1 2
         Authentication type is none
         Split Horizon with poissoned reverse is enabled
         Restrcts default route installation
          Restricts default route origination

6. On switch 2, review the RIP route entries for the static routes that were added in switch 1.

   In switch 1, static routes with the metric of 3 are redistributed into the RIP domain. The following output shows the redistributed static routes with the metric of 4.

       SEFOS# show ip rip database

       10.0.0.0/8  [1]        auto-summary
       10.0.0.0/16 [1]        directly connected, vlan1
       50.0.0.0/8  [4]        auto-summary
       50.0.0.0/8  [4]        via 10.0.0.1, vlan1
       60.0.0.0/8  [4]        auto-summary
       60.0.0.0/8  [4]        via 10.0.0.1, vlan1
       70.0.0.0/8  [4]        auto-summary
       70.0.0.0/8  [4]        via 10.0.0.1, vlan1
       80.0.0.0/8  [4]        auto-summary
       80.0.0.0/8  [4]        via 10.0.0.1, vlan1

7. Review the IP routing table on switch 2.

       SEFOS# show ip route

       C 10.0.0.0/16 is directly connected, vlan1
       C 30.2.2.0/24 is directly connected, vlan3
       R 50.0.0.0/8  [4] via 10.0.0.1
       R 60.0.0.0/8  [4] via 10.0.0.1
       R 70.0.0.0/8  [4] via 10.0.0.1
       R 80.0.0.0/8  [4] via 10.0.0.1

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |