Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure an OSPFv3 Neighbor

In this example, SEFOS1 is the switch on which OSPFv3 is enabled, `10.0.0.1` is specified as the router ID, and `VLAN 10` is configured on the NBMA network with a neighbor priority of 10.

1. Enter Global Configuration mode in SEFOS1.

       SEFOS# configure terminal

2. Enable OSPF globally in SEFOS1.

       SEFOS(config)# ipv6 router ospf

3. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.0.0.1

4. Exit Router Configuration mode.

       SEFOS(config-router)# exit

5. Enter Interface Configuration mode.

       SEFOS(config)# interface vlan 10

6. Configure the network type as NBMA.

       SEFOS(config-if)# ipv6 ospf network non-broadcast

7. Configure the neighbor with priority#10.

       SEFOS(config-if)# ipv6 ospf neighbor fe80::214:4fff:fe6c:d04d priority 10

8. View the SEFOS1 configuration.

       SEFOS# show ipv6 ospf neighbor

       ID            Pri      State           DeadTime       Address
       10.0.0.8        1       FULL/BACKUP       38           fe80::214:4fff:fe6c:d04d

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |