Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure an IPv4 Address for an Interface

The IPv4 address is a 32-bit unique identifier that identifies a host or a destination in a network.

1. Create the interface (`1` in this case).

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 1

2. Configure the IPv4 address on the interface.

       SEFOS(config-if)# ip address 11.0.0.1 255.0.0.0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |