Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

## Display Spanning Tree Information for Active Ports

This command displays the bridge and details of the active ports (ports that are participating in the spanning-tree).

- Type.

      SEFOS# show spanning-tree active

      Root Id         Priority   32768
                      Address    00:01:02:03:04:01
                      Cost       0
                      Port       0 [0]
                      This bridge is the root
                     Max age 20 Sec, forward delay 11 Sec
                      Hello Time is 2
      MST00
      Spanning tree Protocol Enabled.
      MST00 is executing the mstp compatible Multiple Spanning Tree Protocol
      Bridge Id       Priority  32768
                      Address  00:01:02:03:04:01
                     Max age is 20 sec, forward delay is 11 sec
                      Hello Time is 2 sec                Dynamic Path Cost is Disabled                Dynamic Path Cost Lag-Speed Change is Disabled
      Name      Role         State        Cost     Prio   Type
      ----      ----         -----        ----     ----   ------
      Ex0/1     Designated   Forwarding   200000   128    P2P
      Ex0/2     Designated   Forwarding   200000   128    SharedLan

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |