Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## General Configurations

This section contains procedures for configuring RIP in SEFOS. See Configuring the RIP Topology Example for descriptions of the topologies that are referenced in the procedures. Before you can configure RIP, you must configure the switches in your environment. To configure switch 1, see Configure Switch 1. To configure switch 2, see Configure Switch 2, and to configure switch 3, see Configure Switch 3. RIP is disabled by default.

- Managing RIP

- Configuring RIP Security

- Configuring the RIP Packet Retransmission Interval and Retry Count

- Configuring RIP Neighbors

- Configuring the RIP Passive Interface

- Configuring the Output Delay

- Configuring Redistribution

- Configuring the Default Metric

- Managing the `auto-summary` Option

- Configuring Interface-Specific RIP Parameters

- Configuring the Debug Level for RIP

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |