Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure an Interface as an Upstream Interface

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Enable IGMP on the interface if it is not already enabled.

       SEFOS(config-if)# set ip igmp enable

3. Set the interface as an upstream interface.

       SEFOS(config-if)# ip igmp-proxy mrouter
       SEFOS(config-if)# end

4. Ensure that the IP address has changed.

       SEFOS# show ip igmp interface

       ...
        Internet Address is 12.0.0.1/8
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |