Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Restore the Default Transmission Delay

This example restores the default time for transmitting a link state update packet on an interface to 1 second.

- Restore the default transmit delay.

      SEFOS(config-if)# no ipv6 ospf transmit-delay

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |