Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

## Verify the L3 OSPF Configuration

Note - All pings should be successful. Each switch has learned all routes to different networks in the topology through OSPF.

1. Verify the configuration on `Host-1`.

       [Host-1 ~]# ifconfig

       eth1      Link encap:Ethernet  HWaddr 00:10:E0:22:0F:D9
                 inet addr:192.168.20.20  Bcast:192.168.20.255  Mask:255.255.255.0
                 inet6 addr: fe80::210:e0ff:fe22:fd9/64 Scope:Link
                 UP BROADCAST RUNNING MULTICAST  MTU:1500  Metric:1
                 RX packets:107 errors:0 dropped:0 overruns:0 frame:0
                 TX packets:357 errors:0 dropped:0 overruns:0 carrier:0
                 collisions:0 txqueuelen:1000
                 RX bytes:9530 (9.3 KiB)  TX bytes:41674 (40.6 KiB)

       eth1.150  Link encap:Ethernet  HWaddr 00:10:E0:22:0F:D9
                 inet addr:192.168.150.20  Bcast:192.168.150.255  Mask:255.255.255.0
                 inet6 addr: fe80::210:e0ff:fe22:fd9/64 Scope:Link
                 UP BROADCAST RUNNING MULTICAST  MTU:1500  Metric:1
                 RX packets:0 errors:0 dropped:0 overruns:0 frame:0
                 TX packets:63 errors:0 dropped:0 overruns:0 carrier:0
                 collisions:0 txqueuelen:0
                 RX bytes:0 (0.0 b)  TX bytes:8046 (7.8 KiB)

       eth1.151  Link encap:Ethernet  HWaddr 00:10:E0:22:0F:D9
                 inet addr:192.168.151.20  Bcast:192.168.151.255  Mask:255.255.255.0
                 inet6 addr: fe80::210:e0ff:fe22:fd9/64 Scope:Link
                 UP BROADCAST RUNNING MULTICAST  MTU:1500  Metric:1
                 RX packets:0 errors:0 dropped:0 overruns:0 frame:0
                 TX packets:48 errors:0 dropped:0 overruns:0 carrier:0
                 collisions:0 txqueuelen:0
                 RX bytes:0 (0.0 b)  TX bytes:6760 (6.6 KiB)

2. Verify the configuration on `Host-2`.

       Host-2# ifconfig nxge1
       index 41001000843<UP,BROADCAST,RUNNING,MULTICAST,IPv4,FIXEDMTU> mtu 9000 nxge1: flags=
               inet 192.168.30.20 netmask ffffff00 broadcast 192.168.30.255
               ether 0:14:4f:6c:43:9

3. Verify the configuration on `Host-3`.

       [Host-3 ~]# ifconfig
       eth1  Link encap:Ethernet  HWaddr 00:07:E9:04:D1:9F
             inet addr:192.168.50.20  Bcast:192.168.50.255  Mask:255.255.255.0
             inet6 addr: fe80::207:e9ff:fe04:d19f/64 Scope:Link
             UP BROADCAST RUNNING MULTICAST  MTU:1500  Metric:1
             RX packets:240930477 errors:0 dropped:515783109 overruns:0 frame:0
             TX packets:13447642 errors:0 dropped:0 overruns:0 carrier:0
             collisions:0 txqueuelen:1000
             RX bytes:727267562 (693.5 MiB)  TX bytes:564925930 (538.7 MiB)

       eth1.100  Link encap:Ethernet  HWaddr 00:07:E9:04:D1:9F
             inet addr:192.168.100.20  Bcast:192.168.100.255  Mask:255.255.255.0
             inet6 addr: fe80::207:e9ff:fe04:d19f/64 Scope:Link
             UP BROADCAST RUNNING MULTICAST  MTU:1500  Metric:1
             RX packets:0 errors:0 dropped:0 overruns:0 frame:0
             TX packets:66 errors:0 dropped:0 overruns:0 carrier:0
             collisions:0 txqueuelen:0
             RX bytes:0 (0.0 b)  TX bytes:13336 (13.0 KiB)

       eth1.101  Link encap:Ethernet  HWaddr 00:07:E9:04:D1:9F
             inet addr:192.168.101.20  Bcast:192.168.101.255  Mask:255.255.255.0
             inet6 addr: fe80::207:e9ff:fe04:d19f/64 Scope:Link
             UP BROADCAST RUNNING MULTICAST  MTU:1500  Metric:1
             RX packets:0 errors:0 dropped:0 overruns:0 frame:0
             TX packets:36 errors:0 dropped:0 overruns:0 carrier:0
             collisions:0 txqueuelen:0
             RX bytes:0 (0.0 b)  TX bytes:5966 (5.8 KiB)

4. Ping from `Host-3` to untagged and tagged interfaces on `Host-1` of the core switch.

       [Host-3 ~]# ping 192.168.20.20
       [Host-3 ~]# ping 192.168.150.20

5. Ping from `Host-1` to untagged and tagged interfaces on `Host-3` of `ES1-24p-1`.

       [Host-1 ~]# ping 192.168.50.20
       [Host-1 ~]# ping 192.168.100.20

6. Ping from `Host-1` to an untagged interface on `Host-2` of `ToR72p-1`.

       [Host-1 ~]# ping 192.168.30.20

##### Related Information

- Configure Switch `TOR72p-1` for L3 Routing Using OSPF

- Configure Switch `TOR72p-2` for L3 Routing Using OSPF

- Configure Switch `ES1-24p-1` for L3 Routing Using OSPF

- Configure Switch `ES1-24p-2` for L3 Routing Using OSPF

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |