Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure SEFOS3

Use the following commands to configure `VLAN 20` and `VLAN 30` on SEFOS3 in the example topology.

1. Configure SEFOS3.

       SEFOS 3 SEFOS# configure terminal
       SEFOS 3 SEFOS(config)# set gvrp disable
       SEFOS 3 SEFOS(config)# set gmrp disable

       SEFOS 3 SEFOS(config)# interface extreme-ethernet 0/65
       SEFOS 3 SEFOS(config-if)# no shutdown
       SEFOS 3 SEFOS(config-if)# switchport access vlan 20
       % Access VLAN does not exist.,Creating vlan
       SEFOS 3 SEFOS(config-if)# exit

       SEFOS 3 SEFOS(config)# interface vlan 20
       SEFOS 3 SEFOS(config-if)# no shutdown
       SEFOS 3 SEFOS(config-if)# ipv6 enable
       SEFOS 3 SEFOS(config-if)# ipv6 address 2222::13 112
       SEFOS 3 SEFOS(config-if)# exit

       SEFOS 3 SEFOS(config)# vlan 30
       SEFOS 3 SEFOS(config-vlan)# port extreme-ethernet 0/1
       SEFOS 3 SEFOS(config-vlan)# exit

       SEFOS 3 SEFOS(config)# interface extreme-ethernet 0/1
       SEFOS 3 SEFOS(config-if)# no shutdown
       SEFOS 3 SEFOS(config-if)# exit

       SEFOS 3 SEFOS(config)# interface vlan 30
       SEFOS 3 SEFOS(config-if)# no shutdown
       SEFOS 3 SEFOS(config-if)# ipv6 enable
       SEFOS 3 SEFOS(config-if)# ipv6 address 3333::13 112
       SEFOS 3 SEFOS(config-if)# end

2. Show the status of the IPv6 interface on SEFOS3.

       SEFOS 3 SEFOS# show ipv6 interface
       vlan1 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::214:4fff:fe6c:686d
           Global unicast address(es):
               Not Configured.
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::1:ff6c:686d
           MTU is 9216
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled
       vlan20 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::214:4fff:fe6c:686d
           Global unicast address(es):
               2222::13/112
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::9
               ff02::1:ff00:13
               ff02::1:ff6c:686d
           MTU is 9216
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled
       vlan30 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::214:4fff:fe6c:686d
           Global unicast address(es):
               3333::13/112
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::9
               ff02::1:ff00:13
               ff02::1:ff6c:686d
           MTU is 9216
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled

       SEFOS 3 SEFOS#

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |