Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LA Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the LACP Port Identifier

In the following procedure, ports 0/1, 0/2, and 0/3 are part of the LA.

1. On switch A, review the port state behavior for the default port identifier.

       SEFOS# show etherchannel 1 detail

   The following output has been truncated for readability.

       ...
                        LACP Port   Admin  Oper   Port    Port
       Port     State   Priority    Key    Key    Number  State
       ---------------------------------------------------------------------
       Ex0/1    Bundle  128         1      1      0x1     0xbe
       Ex0/2    Bundle  128         1      1      0x2     0xbe
       Ex0/3    Standby 128         1      1      0x3     0xa2
       ...

   Note - Before you configure the LACP port identifier, note that the `extreme-ethernet` port, `0/3`, in switch A and switch B are standby ports.

2. For port 0/3 in switch A, configure the port identifier as 1.

       SEFOS(config)# interface extreme-ethernet 0/3
       SEFOS(config-if)# lacp port-identifier 1

3. Review the configuration information.

   The output has been truncated for readability.

       SEFOS# show etherchannel detail

       ...
                        LACP Port   Admin  Oper   Port    Port
       Port     State   Priority    Key    Key    Number  State
       ---------------------------------------------------------------------
       Ex0/1    Bundle  128         1      1      0x1     0xbc
       Ex0/2    Standby 128         1      1      0x2     0xa0
       Ex0/3    Bundle  128         1      1      0x3     0xbc
       ...

   Note - After you configure the LACP port identifier, note that the `extreme-ethernet` port, 0/3, in switch A is brought up in the bundle state.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |