Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Restore the Default Redistribution Configuration

The following example deletes the external LSA generated for `3333::1111:0:0`, and a new external LSA is generated with the default redistribution configuration.

1. Test `no redist-config` in SEFOS1.

       SEFOS# configure terminal
       SEFOS(config)# ipv6 router ospf

2. Restore the default redistribution configuration.

       SEFOS(config-router)# no redist-config 3333::1111:0:0 96
       SEFOS(config-router)# end

3. View the configuration details in SEFOS1.

       SEFOS# show ipv6 ospf database as-external detail

       Age: 0   Seconds            LS Type: External Lsa
       Link State Id: 0.0.0.1      Adv Rtr Id: 10.0.0.1
       Sequence: 0x80000006        Checksum: 0x947e    Length: 56
       Metric Type: Ext Type2      Metric: 0xa
       Prefix Length: 96            Prefix Options: 0x00
       Referenced LS Type: 0
       Addres Prefix: 3333::1111:0:0
       Fw Addres Prefix: 3333::1111:fec0:0
       External Route Tag: 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |